KEMENTERIAN AGAMA

**UNIVERSITAS ISLAM NEGERI MAULANA MALIK IBRAHIM MALANG**

#### FAKULTAS SAINS DAN TEKNOLOGI

Jalan Gajayana 50 Malang 65144 Telepon/ Faksimil (0341) 558933

Nomor : Un.03/KS.01.04/3468/2013 21 Oktober 2013

Lampiran : 1 bendel

Hal : Permintaan Informasi Harga Barang

Kepada

Yth. ..........................................................

Di Tempat

*Assalamu’alaikum Wr. Wb.*

Dengan hormat, sehubungan rencana realisasi pelaksanaan pekerjaan ***Belanja Modal Peralatan dan Mesin Jurusan Biologi dan Matematika Fakultas Sains dan Teknologi***(kode 2132.997.001.016 MAK 532111), maka kami bermaksud agar perusahaan saudara memberikan informasi tentang harga barang sesuai dengan Rencana Anggaran Biaya (RAB) yang kami lampirkan dalam surat ini.

Apabila informasi harga yang saudara berikan sesuai dan kami nilai wajar, maka kami akan memberikan kesempatan perusahaan saudara untuk membuat penawaran terhadap pekerjaan tersebut.

Kami harap data barang dan harganya dapat kami terima paling lambat pada:

Hari/ Tanggal : Rabu/ 23 Oktober 2013

Waktu : 12.00 WIB

Tempat : Fakulktas Sains dan Teknologi UIN Maliki Malang atau dikirim via e-mail ke: [ulp@uin-malang.ac.id](mailto:ulp@uin-malang.ac.id) atau [ulp\_uinmalang@kemenag.go.id](mailto:ulp_uinmalang@kemenag.go.id)

Surat tentang informasi harga barang tersebut, ditujukan:

Kepada

Yth. Pejabat Pembuat Komitmen Fakultas Sains dan Teknologi

UIN Maulana Malik Ibrahim Malang

Demikian atas perhatian dan kerjasamanya, kami sampaikan terima kasih.

*Wassalamu’alaikum Wr. Wb.*



Lampiran Surat

Nomor : Un.03/KS.01.04/3468/2013

Tanggal : 21 Oktober 2013

Tentang :

***Belanja Modal Peralatan dan Mesin***

***Jurusan Biologi dan Matematika Fakultas Sains dan Teknologi***

(kode 2132.997.001.016 MAK 532111

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **No** | **Nama Barang** | **Spesifikasi** | **Volume** | **Harga Satuan** | **Total Harga** |
|  | Lemari Es | • Product Type: 2 door Frost Free • Product Installation: Free Standing • Energy Class: 5 stars • Frequency (Hz): 60 • Voltage (v): 230 • Climate Class: T • Control Settings: knob • Type of Control: Electronic • Number of Compressors: 1 • Shelves Material: Tempered Glass • No. of Shelves: 2 • Number of Cooling Systems: 1 • Freezer Defrost Process: Automatic, Frost free • Adjustable Feet: Yes • Freezer Net Capacity (l): 61.7 • Refrigerator Net Capacity (l): 147.8 • Plug Type: EU • Ventilator: Yes • Door Hinge: Right • Net Capacity: 209.5 • Dimensions (H x W x D): 1405 x 540 x 615mm | 1 Unit | .................. | ...................... |
|  | Exaust Fan | Excellent Performance in Moisture & Smell Exhaust Compact & Stylish Easy Installation Trace-Prevention Feature & Back Draft Shutter Feature 8" (12 cm) | 1 Unit | .................... | ....................... |
|  | Tabung Nitrogen | Kapasitas : 6 M2 | 1 Unit | ................... | ....................... |
|  | Stamfolt | 500 Watt, 1 Phase | 1 Unit | ................... | ........................ |
|  | UV Lamp | Wattage: 4 Watts  Wavelength: 366 nm  Batteries: 5 x 1.5 V baby cells  Weight: Approximately 400 g  Dimensions: 16 x 9 x 2.5 cm | 1 Unit | ................... | ....................... |
|  | CCTV | |  |  | | --- | --- | | **Camera Box Waterproof 8 pcs** | | | ▪ Reolotion : 380 TVL / 540 TVL | | | ▪ Color : 0.01 Lux at F1.2 / 0.03 Lux at F1.2 | | | ▪ Special Circuit to Avoid Color Rolling | | ▪ 3-Axis Camera Construction | | | ▪ Optically Perfect Impact and Dust Resistant Polycarbonate Dome Cover | | | ▪ Screw-on Design Dome Cover for Easy and Secure Installation | | | ▪ RCA Video Connector for Easy Adjustment on Site | | | ▪ 4~9 mm Lens option | | | **DVR 8 Channel**  DVR 8 CHANNEL Audio Input / Output ( CH) : RCA 8 / 1 Display Rate: D1@ 30/ 25( FPS/ CH)  Recording Rate( MAX) ( FPS)  CIF 240 / 200 D1 120/ 100 ( 2CHxD1 real time, 6CHxCIF real time)  Playback Rate  CIF 120/ 100 ; D1 240 / 200 Playback Channel( Multiple channels) : 1, 4, 8 Resolution Preview PAL D1 704 x 576 Recording PAL D1 704 x 576, Half D1 704 x 288, CIF 352X 288 Networking | | | TCP / IP, UDP, DHCP, DNS, PPPOE, DDNS, Email, Alarm Server, UPNP Backup Device Flash Driver, USB HDD, USB DVD-RW, Network download Mobile Phone / PDA Symbian, Windows Mobile, iPhone, Google Android, Blackberry Hard disk driver SATA × 2( MAX 4TB) | | | | **Instalasi** | | |  | ................... | ....................... |
| **TOTAL** | | | | | **.......................** |



